# IP Media Processor circuit pack

The IP Media Processor circuit pack supports transmission of voice data over an IP network. Thereby, the IP Media Processor circuit pack can support applications that comply with the H.323-v2 protocols. IP Media Processor offers a lower per-port cost and improved quality through use of dynamic jitter buffers. In addition, IP Media Processor circuit pack performs echo cancellation, silence suppression, Dual Tone Multi-Frequency (DTMF) detection, and conferencing.

The IP Media Processor circuit pack provides Voice over Internet Protocol (VoIP) for Avaya one-X Agent. You can use the IP Media Processor circuit pack for My Computer, Office Phone, and Other Phone configurations, where the system establishes a VoIP connection with Communication Manager.
Note

For installation procedures and configuration information on C-LAN and IP Media Processor circuit packs, see Administering Network Connectivity on Avaya Aura Communication Manager on the Avaya Support Site at http://www.avaya.com/support.

Parent topic: Communication Manager circuit packs
©2011, Avaya Inc. All Rights Reserved.