# Creating the Touch Tone shortcuts

Use the following steps to create a Touch-Tone number and to use it as a shortcut in the Dial Pad window. A typical use can be to store a DTMF login to a voice mailbox, or to execute DTMF in band Network Call Transfer functions provided by the network service provider.

1. From the top bar, select Settings > System Settings.
2. On the left of the System Settings dialog box, click Touch-Tone Shortcuts.
3. Click Add.

   The system displays an untitled item in the Touch-Tone Shortcuts list.

4. In the Touch Tone Shortcuts list, double-click the Untitled item and specify the touch-tone shortcuts name.
5. In the Phone Number field, enter a valid telephone number and include * or #.

   The phone number can be an extension number, a PSTN number, or a mobile number.

6. Click OK and close the System Settings window.

   The system saves the touch-tone number in the Touch-Tone Shortcuts list. The new telephone number will be available as a Touch-Tone Shortcut in the dialpad window.

Related information
Touch Tone Shortcuts panel field descriptions
©2011, Avaya Inc. All Rights Reserved.