## Web Configuration Tool

Recent call server versions provide all the Web configuration support the 9600 Series IP Telephones require. Also, the media server has an easy to use, PC-based interface for creating script files. Given these resources, you do not need to manually create the text files discussed in 9600 Series IP Telephone Scripts and Application Files. For more information about the media server, see Installation and Upgrades for Avaya G700 Media Gateway and Avaya S8300 Media Server, available on the Avaya support Web site.

Table 7: 9600 Series IP Telephone Customizable System Parameters lists the parameters you can administer when manually creating the configuration file. Manual administration is discussed in 9600 Series IP Telephone Scripts and Application Files. When using the media server, you do not need to know the specific parameter names, since the media server handles that. For more information, Table 6 lists the parameter names from 9600 Series IP Telephone Customizable System Parameters and the corresponding field name from the media server HTTP server application. Any limits, restrictions, etc. about the parameters are built into the media server.

NOTE: The Web Configuration application covers other IP telephones. This document covers only data applicable to 9600 Series IP Telephones.

Table 6: Media Server Field Names & Corresponding Script File Parameter
Names
Media Server Field Name | Script File Parameter Name
--- | ---
Script File Server Authentication. Note: Applicable only when configuration file downloaded using HTTPS. Not applicable if file downloaded using HTTP. | AUTH
DHCP Lease Violation Flag | DHCPSTD
Domain Name | DOMAIN
Domain Name Server | DNSSRVR
HTTP Server IP Address | HTTPSRVR
HTTP Directory | HTTPDIR
Source IP Addresses for SNMP Queries | SNMPADD
SNMP Community String | SNMPSTRING
Telephone Country Code | PHNCC
Telephone Dial Plan Length | PHNDPLENGTH
International Access Code | PHNIC
Long Distance Access Code | PHNLD
National Telephone # Length | PHNLDLENGTH
Outside Line Access Code | PHNOL
Local Dialpad Procedures Allowed | PROCSTAT
Handset Audio Gain Control Status | AGCHAND
Headset Audio Gain Control Status | AGCHEAD
Speaker Audio Gain Control Status | AGCSPKR
Application Status | APPSTAT
CNA Server Addresses | CNASRVR
CNA Port Number | CNAPORT
802.1X Supplicant Mode | DOT1X
Send Destination Unreachable Messages | ICMPDU
Process Received Redirect Messages | ICMPRED
Layer 2 Frame Tagging | L2Q
802.1A VLAN Identifier | L2QVLAN
System-Wide Language | LANGSYS
English Language Selection Status | LANG0STAT
Event Log Security Level | LOGLOCAL
Syslog Server Address | LOGSRVR
Management Complex IP Addresses | MCIPADD
Voice Mail Telephone Number | MSGNUM
Wait Time for DHCP Offer | VLANTEST
Ethernet Line Interface Status | PHY1STAT
Secondary Ethernet Interface Layer 2 Priority Value | PHY2PRIO
Secondary Ethernet Line Interface Status | PHY2STAT
Secondary Ethernet Interface VLAN Identifier | PHY2VLAN
Local (dial pad) Procedure Password | PROCPSWD
Reregistration Timer | REREGISTER
RTCP Monitor IP Address | RTCPMON
Subscription List | SUBSCRIBELIST
Trusted Domains/Paths | TPSLIST
Unnamed Registration Status | UNNAMEDSTAT
Secondary Ethernet Interface Layer 2 Frame Tagging | VLANSEP
9600 Home Page | WMLHOME
9600 HTTP Proxy Server | WMLPROXY
9600 HTTP Proxy Server Port | WMLPORT
9600 HTTP Proxy Server Exception Domains | WMLEXCEPT
Idle Time Before Web Page Display | WMLIDLETIME
Idle Time Web Page Display | WMLIDLEURI
Idle Time Before Backlight Turnoff | BAKLIGHTOFF
Backup and Restore URI | BRURI
User Options Access | OPSTAT