## About Local Administrative Procedures

Local administrative procedures allow you to customize the 9600 Series IP Telephone installation for your specific operating environment. This section provides a description of each local administrative option covered in this guide, with references to the pages on which the option appears.

NOTE: Unless otherwise prohibited by administration, the user can view but not change most of the parameters associated with Local Administrative procedures. For more information about this option, see the applicable user guides.

Local Programming Option | Code | See
--- | --- | ---
Set 802.1X operational mode | 8 0 2 1 X (8 0 2 1 9) | Set the 802.1X Operational Mode.
Static addressing | A D D R (2 3 3 7) | Static Addressing Installation.
Automatic Gain Control | A G C (2 4 2) | Disable/Enable Automatic Gain Control.
DHCP chaddr field value | C H A D D R (2 4 2 3 3 7) | Manually Setting the DHCP Client Hardware Address.
Clear values to factory defaults | C L E A R (2 5 3 2 7) | Clear Procedure.
Enable/disable Debug Mode | D E B U G (3 3 2 8 4) | Disable/Enable Debug Mode.
Group Identifier | G R O U P (4 7 6 8 7) | Group Identifier.
Interface Control | I N T (4 6 8) | Interface Control.
Event Logging | L O G (5 6 4) | Disable/Enable Event Logging.
System-specific Logoff | L O G O F F (5 6 4 6 3 3) | Logoff.
Reset the telephone | R E S E T (7 3 7 3 8) | Reset System Values.
Restart the telephone | R E S E T (7 3 7 3 8) | Restart the Telephone.
Signaling protocol identifier (not applicable to Release 1.0) | S I G (7 4 4) | Signaling Protocol Identifier.
Site-Specific Option number | S S O N (7 7 6 6) | Site-Specific Option Number Setting.
Test the telephone | T E S T (8 3 7 8) | Self-Test Procedure.

NOTE: Unless otherwise prohibited using administration, the user can view but not change most of the parameters associated with Local Administrative Procedures. For more information about this option, see the applicable user guide(s).