## Group Identifier

Use the following procedure to set or change the Group Identifier.

NOTE: Perform this procedure only if the LAN Administrator instructs you to do so.
For more information about groups, see The GROUP System Value.

While the telephone is on-hook and idle, press the following sequence of keys on the faceplate of the telephone:

Mute 4 7 6 8 7 (Mute G R O U P)

NOTE: Press the Mute button momentarily. Do not press this button while pressing other keys/buttons.

The following text displays left-justified at the top of the display:

Group=ddd New=_

where ddd is the Group value.

1. Enter a valid Group value (0-999).

If a value different from the current Group value is entered, the following text displays left-justified at the top of the display:

Save new value? *=no #=yes

1. Press the * button to terminate the procedure, or the # button to save the new value.

If you press the # button, the following text displays:

New value being saved

The new value is saved and the user interface is restored to its previous state.