#### Pushable vs. Non-Pushable States

The following are non-pushable states for Display pushes to an IP telephone:

- When the user is in text entry mode on a Web text entry screen or Contacts text entry screen (for normal priority only).
- When the telephone is in the process of restoring a retrieved backup file.
- When a Local Procedure has been initiated.

If a phone is not in one of the above states, it is considered to be in a pushable state, meaning the telephone will accept a pushed message.