## Entering Data for Administrative Options

This section applies to all 9600 Series IP Telephones and describes how to enter data for administrative options.

1. Invoke all local procedures by pressing the Mute button, up to 7 numeric dial pad buttons, and the # button.

A 6-second timeout is in effect between button presses after pressing the Mute button. If you do not press a valid button within 6 seconds of pressing the previous button, the collected digits are discarded. In this case, no administrative option is invoked.

1. Attempts to enter invalid data are rejected, and the telephone emits an error beep.
2. If you enter a numeric digit for a value or for an IP address or subnet mask field after entering only a zero, the new digit replaces the zero.
3. Press the # button to go to the next step.
4. To backspace, press the leftmost softkey. When you press the applicable button or key to backspace, the most recently entered digit or period is erased from the display. The cursor remains in the erased character’s former position.
5. If PROCPSWD is administered as indicated in Chapter 7 of the Avaya one-X Deskphone Edition for 9600 Series IP Telephones Administrator Guide, you must type the Local Procedure password after pressing Mute and before pressing the code for your given local programming option.

NOTE: If PROCSTAT has been administered to 1, you will not be able to invoke any administrative options other than V I E W.