### Priorities and States

Normal and barge priorities are not applicable to the Subscribe push type.

The Subscription service is initialized during registration or the IP telephone boot-up process. Once the telephone is properly registered (logged in) with the media server, the telephone subscribes to the server listed in the SUBSCRIBELIST parameter.

NOTE: For more information on SUBSCRIBELIST and boot-time subscription service, see Chapter 4: Push Administration.