## Logoff

Use the following procedure to log off a telephone.

CAUTION: Once a telephone is logged off, a password and extension might be needed to log back on.

1. While the telephone is on-hook and idle, press the following sequence of keys on the faceplate of the telephone:

Mute 5 6 4 6 3 3 # (Mute L O G O F F #)

NOTE: Press the Mute button momentarily. Do not press this button while pressing other keys/buttons.

1. After entry of the command sequence, the telephone unregisters from the call server. The telephone display (and button module display, if applicable) clears, then displays the following prompt for subsequent login:

Login
Enter Extension
Enter Extension and press Enter or OK