## Disable/Enable Event Logging

Use the following procedure to enable or disable logging of system events.

1. While the telephone is on-hook and idle, press the following sequence of keys on the faceplate of the telephone:

Mute 5 6 4 # (Mute L O G #)

NOTE: Press the Mute button momentarily. Do not press this button while pressing other keys/buttons.

1. After entry of the command sequence, the telephone displays the following text, depending on the current value of the system parameter NVLOGSTAT:

Log=status *=change #=OK

where status is the type of logging indicated by the NVLOGSTAT value, defined as:

- Status is disabled when NVLOGSTAT = 0
- Status is emergencies when NVLOGSTAT = 1
- Status is alerts when NVLOGSTAT = 2
- Status is critical when NVLOGSTAT = 3
- Status is errors when NVLOGSTAT = 4
- Status is warnings when NVLOGSTAT = 5
- Status is notices when NVLOGSTAT = 6
- Status is information when NVLOGSTAT = 7
- Status is debug when NVLOGSTAT = 8

1. To change the logging status, press *.

Depending on the current value, the next sequential valid NVLOGSTAT value is selected and displayed as the status. For example, if the current value is alerts (2), pressing * changes the value to 3 (critical). If the current value is debug (8), pressing * changes the value to 0 (disabled).

If a value different from the current NVLOGSTAT value is entered, the following text displays left-justified at the top of the display:

Save new value? *=no #=yes

1. Press the * button to terminate the procedure, or the # button to save the new value. If you press the # button, the telephone displays the following text:

New value being saved

The telephone saves the new value.