### Powering the 9600 Series IP Telephone

All 9600 Series IP Telephones can be locally powered with a Telephone Power Module (DC power jack), available separately. In addition, the telephones support IEEE 802.3af-standard LAN-based power. Before installing a 9600 Series IP Telephone, verify with the LAN administrator whether the LAN supports IEEE 802.3af, and if so, whether the telephone should be powered locally or by means of the LAN.

NOTE: The last step in assembling the 9600 Series IP Telephone must be applying power. Apply power either by plugging the power cord into the power source (local powering) or plugging the modular line cord into the Ethernet wall jack (IEEE powering).

CAUTION: Failure to connect the proper cables with the proper jacks might result in an outage in part of your network.

Figure 1 and Figure 2 provide illustrations to connect cords to jacks on 9600 IP Series Telephones. Use the illustrations and associated procedures as appropriate for telephone assembly.

Telephone Model: | See:
9620 | Figure 1
9630 | Figure 2

Figure 1: Connection Jacks on a 9620 Series IP Telephone

Figure 2: Connection Jacks on a 9630 Series IP Telephone

1. Plug one end of the H4DU 4-conductor coiled handset cord into the telephone and the other end into the handset.
2. Plug one end of the first Category 5 modular line cord into the Ethernet jack of the PC and the other end into the secondary Ethernet jack on the 9600 Series IP Telephone,
   if appropriate.
3. Plug one end of the second Category 5 modular line cord into the Ethernet jack on the 9600 Series IP Telephone. Plug the other end of this cord into the Ethernet wall jack. If the telephone is to be IEEE-powered, you are finished. Do not proceed to Step 4.
4. If the telephone is to be powered locally in the United States and Canada, plug the power cord into the 9600 Series IP Telephone, and the power cord plug into the wall socket.

If the telephone is to be powered locally outside the United States and Canada, connect the 1151 power brick to the power cable. Connect the other end of the power cable to the 9600 Series IP Telephone, and the plug to the wall socket.