#### Pull operation (Step 2a and Step 2b)

The phone requests the target URI of the Push Content from a Trusted Push Server. The Push Content can be any valid WML file or an XML file with tags that instruct the endpoint to do one or more of the following:

- Set up an RTP audio stream,
- Display a message on the Top Line,
- Display a full screen message with images and links, or
- Re-subscribe with the subscription server.