## Chapter 8: Administering Applications and Options

## Customizing 9600 Series IP Telephone Applications and Options

The 9600 Series IP Telephones have some unique and powerful capabilities that take advantage of their display and access to LAN facilities. If your LAN has a WML Web site, the telephone needs key information about the servers providing those facilities. You need to provide the information called for in relevant sections of Table 11 in a customized script file. For more information, see 9600 Series IP Telephone Scripts and Application Files.

CAUTION: For the telephones to work properly, you must have a 46xxsettings.txt file in the same directory as the application file. If you do not edit the 46xxsettings.txt file, those telephones use default settings only. The 46xxsettings file is available as a standalone download. If you already have such a file because you downloaded it for a previous 9600 Series or 4600 Series IP Telephone release, installing the standalone file overwrites the original file.

NOTE: To facilitate administration, the 9600 Series and 4600 Series IP Telephones use the same 46xxsettings.txt file.

In Table 11, parameters shown with a Mandatory status must be accurate and non-null for the application to work. You can change parameters with an Optional status to suit your environment. If you do not change parameters, the defaults are used.

Table 11: 9600 Series IP Telephone Customizable System Parameters
Parameter Name | Default Value | Status | Description and Value Range
--- | --- | --- | ---
General User Parameters:
APPSTAT | 1 | Optional | Applications status flag. See The Application Status Flag (APPSTAT) for a description. See Table 12 for the range of values.
OPSTAT | 111 | Optional | Options status flag(s) (1 or 3 ASCII numeric digits) indicate which options are user-selectable. The default of 111 grants access to all options and related applications. Single digit valid values are: 1=user can access all options, including Logout, 2= user can access only view-oriented applications. Three-digit valid values are a concatenation of binary values, in the form abc, where each letter represents a 0 (disabled/off) or 1 (enabled/on), interpreted as: a = base settings for all user options and related applications, except as noted in b or c. b = setting for view-oriented applications (for example, the Network Information application), as applicable. c = setting for Logout application, if applicable. The binary "0" does not allow an end user to see or invoke options and related applications. The binary "1" allows full display and access to all options and related applications.
Web Access Application Parameters:
SUBSCRIBELIST | " " (Null) | Optional | Subscription list for potential pushed content. List of zero or more fully qualified URLs, separated by commas without intervening spaces, with up to 255 total characters.
TPSLIST | " " (Null) | Optional | List of Trusted Push Servers. List of zero or more fully qualified domain/path strings, separated by commas without intervening spaces, with up to 255 total characters. For more information, see the 4600 Series IP Telephone Application Programmer Interface (API) Guide (Document Number 16-300256).
WMLHOME | " " (Null) | Mandatory | Text string containing the URL of the home page for the Web Access application.
WMLPROXY | " " (Null) | Optional | Text string containing the IP address, in dotted decimal or DNS format, of an HTTP proxy server. This parameter is optional if the Web pages a user accesses are all on the intranet of your organization.
WMLEXCEPT | " " (Null) | Optional | Text string containing a list of one or more HTTP proxy server exception domains, separated by commas, up to a total of 127 ASCII characters. This parameter is optional if the Web pages to be accessed by the user are all on the intranet of your organization. If WMLPROXY is null, the value of this parameter is ignored.
WMLPORT | 80 | Optional | Text string containing the TCP port number for the HTTP proxy server. The default is the TCP default for HTTP. This parameter is optional if the Web pages to be accessed by the user are all on the intranet of your organization. If WMLPROXY is null, the value of this parameter is ignored.
Backup/Restore Parameters
BRURI | " " (Null) | Mandatory | URL used for backup and retrieval of user data. Specify HTTP server and directory path to backup file. Do not specify backup file name. Value: 0-255 ASCII characters. Null is a valid value and spaces are allowed. If this value is null or begins with a character sequence other than http:// or https:// the Backup/Restore option will not display to the telephone user.
Backlight Parameters
BAKLIGHTOFF | 120 | Optional | Number of idle minutes after which the backlight turns off (1-3 ASCII digits, from 0-999).

NOTE: The 4600 Series IP Telephones Application Programmer Interface (API) Guide (Document Number 16-300258) provides assistance in developing local Web sites.