## Troubleshooting

Most problems with the Avaya IP Telephone File Server Application tools are usually configuration- or network-related. A comprehensive set of log files residing in the relevant log directory can help pinpoint any configuration mismatches.

If you want more detailed logging, set the detail log flag to 1 in the MV_IPTel.ini file. Although detailed logging increases output data significantly, it provides a good level of detail for all activities.

Use these steps to help troubleshoot problems:

1. Is the daemon you are trying to access running? First verify that the Avaya IP Telephone File Server Application server is running by launching a Web browser and pointing it to the built-in HTTP server. By default, these run on port 6090 for the Avaya IP Telephone File Server Application daemon, 6091 for MV_WatchDog and 6099 for MV_Manager. For more information, see Checking Application Status. Check that the port hasn’t been changed. For Linux, use the ps –ef | grep MV Linux command or the graphical Services tool in Gnome or KDE. For Windows, check the Service list in the control panel.
2. For Linux, ensure that old versions are not running in parallel. Check using ps –ef | grep MV. Old versions might run in parallel if the daemons are started and stopped without using the scripts provided.
3. Are the standard file locations being used? If not, is the INI file set correctly? Any changes require a server restart to become effective. Use the tools available to check the settings in detail.

NOTE: The current default configuration does not activate either the HTTPS or FTPS servers. At the time of release these functions were unavailable in the IP telephones.

1. If SNMP is not working, ensure that the File Server application server is referenced in
   the 46xx settings file for SNMP. For more information, see the Avaya one-X Deskphone Edition for 9600 Series IP Telephones Administrator Guide or the 4600 Series IP Telephone Administrator Guide as applicable, both available on the Avaya support Web site
   http://www.avaya.com/support. Ensure that the NetSNMP package is available on Linux by issuing an SNMPGET command. For more information, see the SNMP section of the INI file. For example:

smnpget –v2c –cpublic phone-ip-addr .1.3.6.1.4.1.6889.2.69.1.4.9.0

Ensure that the get command returns a valid extension for the IP address used.

1. Ensure that the file system has the correct permissions, particularly on a Linux server. Windows defaults are usually acceptable. Permissions are installed correctly by default, but can be changed manually.
2. Use the built-in facilities/logging of the File Server application to verify whether the HTTP functions are working. The watchdog provides a comprehensive check.
3. Ensure that the server has the correct networking setup and that any firewall functions are not preventing connection to the File Server application server. Ensure that you can access the server over the network. Do this by launching a browser and accessing the HTTP status server, as covered in Checking Application Status. Test files are installed in the HTTP servers.

For HTTP: http://hostname:81/test.html and http://hostname:81/test.zip

For HTTPS: https://hostname:4111/test.html and https://hostname:411/test.zip

NOTE: For HTTPS checks, ensure that you select SSLV2 + SSLV3 as options for this test. Many browsers do not support the security algorithms used in the Avaya IP Telephone File Server Application for TLSV1 and SSLV3.