#### Normal Priority

When the mode attribute in the <Push> tag is set to normal, the telephone state for the Top Line push type is as follows:

- If the Top Line is being used for system messages such as application help messages, then the text string is buffered until the higher-priority message is complete.
- If the phone is in a non-pushable state, meaning the Push Message cannot be displayed on the top display line, the Push Agent sends the Push Initiator the following responses for a normal priority Top Line push request. The Push request does not proceed to request Push Content.

Parameter | Status Code | Reason Phrase
HTTP Status Code | 200 | “OK”
x-Push-Status | 205 | “Not In Push State: Push Aborted”

If a text string is pushed while the top display line is displaying an earlier pushed text string, then the new text string replaces the previous one as a normal priority.

NOTE: The expiration time on all pushed text strings is 30 seconds. All Top Line messages are discarded after 30 seconds.