### New Customizeable System Parameters

In addition to the parameters the preceding table describes and other parameters that the 4600 Series IP Telephones already support, you can set these new parameters in a 46xxsettings.txt file. For more information, see the Avaya one-X Deskphone Edition for 9600 Series IP Telephones Administrator Guide.

New Customizeable System Parameters for 9600 Series IP Telephones
Parameter | Description
--- | ---
BRURI | The URI of the HTTP server used for backup and restore of user data. A subdirectory can be specified, for example:
    SET  BRURI  http://135.8.60.10/backup
This puts the user backup/restore files in a subdirectory away from all other files (.bins, .txts, etc.) and permits authentication to be turned on for that subdirectory, without turning it on for the root directory.
MSGNUM | Voice Messaging system extension number.
BAKLIGHTOFF | The number of minutes of inactivity after which the display backlight turns off. The default is 120 minutes (2 hours). Valid values range from zero (never turn off) to 999 minutes (16.65 hours). This value is supported in the 4625.
SCREENSAVERON | The number of minutes of inactivity after which the telephone displays the screen save. The default is 240 minutes (4 hours). Valid values range from zero (disabled) to 999 minutes (16.65 hours).
WMLIDLETIME | The number of minutes of inactivity after which the Web browser will be displayed if WMLIDLEURI is not null; the default is 10 minutes. Valid values range from 1 to 999 minutes (16.65 hours). This value is supported in the 4625.
WMLIDLEURI | The URI of the Web page to be displayed when the Web browser is displayed due to WMLIDLETIME minutes of inactivity. This value is supported in the 4625.