## Wide Band Codecs

You must administer wide band codecs for each IP codec set and for IP network regions.

Figure 9: IP Codec Set Form

Figure 10: Inter-Network Region Connection Management Form

The entries on the IP address network map shown in Figure 11 might redirect endpoints into a particular network region. That region could be different from what is administered on the previous forms.

Figure 11: IP Address Mapping Form