#### Verifying Your Configuration

This section describes how to verify that the 96XXOPTIONs are correctly configured for the Windows NT® 4.0 DHCP server.

NOTE: Although this configuration represents that for 9600 Series IP Telephones, the file remains as 46XXOPTIONS. This allows shared use for both 4600 and 9600 Series IP Telephones.

##### Verify the Default Option, 242 96XXOPTION

1. Select Start-->Programs-->Admin Tools-->DHCP Manager.
2. Expand Local Machine in the DHCP servers window by double clicking until the + sign changes to a - sign.
3. In the DHCP servers frame, click the scope for the IP telephone.
4. Select Defaults from the DHCP_Options menu.
5. In the Option Name pull-down list, select 242 96XXOPTION.
6. Verify that the Value String box contains the correct string from DHCP Server Administration.

If not, update the string and click the OK button twice.

##### Verify the Scope Option, 242 96XXOPTION

1. Select Scope under DHCP OPTIONS.
2. In the Active Options: scroll list, click 242 96XXOPTION.
3. Click the Value button.
4. Verify that the Value String box contains the correct string from DHCP Generic Setup.

If not, update the string and click the OK button.

##### Verify the Global Option, 242 96XXOPTION

1. Select Global under DHCP OPTIONS.
2. In the Active Options: scroll list, click 242 96XXOPTION.
3. Click the Value button.
4. Verify that the Value String box contains the correct value from DHCP Generic Setup.

If not, update the string and click the OK button.