## Shuffling

Administer shuffling on three forms:

- Feature-Related Parameters form, shown in Figure 6. Set the Direct IP-IP Audio Connections? field to y (yes).
- IP Network Region form, shown in Figure 7. Set both the Intra-region IP-IP Direct Audio field and the Inter-region IP-IP Direct Audio field to y (yes).
- Station form, shown in Figure 8. Set the Direct IP-to-IP Audio Connection to y (yes). The Station form setting overrides the network region, which overrides the system setting.

Figure 6: Feature-Related System Parameters Form

Figure 7: IP Network Region Form

Figure 8: Station Form