### SNMP Configuration of IP Telephones

IP Hardphone software supports configuration parameters allowing control of SNMP servers that can query the IP Hardphones. In a single IP Telephone File Server Application server environment, only the IP address for this server needs to be enabled. But for a High Availability cluster, both real IP addresses and the shared virtual IP address must be enabled.