### Administrable Features

Administrable Station Features
Feature | Administration
--- | ---
Enhanced Conference Features | Administer Conf-dsp (conference display) on the station form as a feature button. Doing so turns on enhanced conference features and gives users advanced conference features.
Call Forward | On the Station form, administer Call Forward as a feature button for the 9630.
Far End Mute | Administer fe-mute (far end mute). When this is enabled the phone shows a “Silence” softkey on the Conference details screen. This feature works only for trunk calls.
Directory Features | Administer Directory, Next, and call-disp (Make Call) on feature buttons for demonstration purposes.
Send All Calls (SAC) | On the Station form, administer SAC (send-calls) as a feature button. On the Station form to the right of where send all calls is administered, leave the extension box empty. This feature requires a coverage path to be administered on the station form.
Coverage Path | For normal operation, you must set up a coverage path for each telephone. Administer the Station form to point to the appropriate system coverage path, for example, coverage path 1.
Auto select any idle appearance | Set Auto select any idle appearance to N (no) to optimize answering calls.
Restrict Last Call Appearance | Set Restrict Last Call Appearance to Y (yes).
Conference/Transfer on Primary Appearance | Set Conference/Transfer on Primary Appearance to Y (yes) to ensure that conference/transfer of a bridged appearance works properly.