Search This CD Index Contact Us
Home > Administration > Networking > AMIS Analog Networking > AMIS Analog Networking Administration > Administering a Loopback Test Machine
| Administering a Loopback Test Machine
> 1. If a remote subscriber sends an AMIS message to this mailbox, the local system sends a copy of the message to the incoming mailbox of the remote subscriber to indicate the message was received. The local loopback test mailbox keeps a copy of the message header in its outgoing mailbox. To administer a loopback test mailbox: Log in to the INTUITY AUDIX Command Prompt. The system displays the AUDIX Command Prompt after you enter your login. At the `enter command:` prompt, enter add subscriber subscriber name where subscriber name is a name that is not defined for any other subscriber (for example, you might use the name "loopback"). The system displays the Add Subscriber screen, page 1. Type an unused local extension in the `Extension`: field.
>    Note: Make a note of this extension. You must enter the same extension number on the System Parameters Analog-Network screen when you administer message delivery parameters.
Press F3 (Enter). Continue with Administering Analog Networking Parameters. Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.