Search This CD Index Contact Us
Home > Alarm Management Window
| Alarm Management Window
> ## Alarm Management Window
> Field | Description
> --- | ---
> Product ID | This is a 10-digit number used to identify the system.
> Alarm Destination | The telephone number the system dials to reach the remote maintenance center. In addition to number the field may include an equal sign (=) which means to wait for a dial tone, or a dash (-) which means to pause for 2 seconds.
> Alarm Origination | When this is active the system notifies the remote maintenance center of alarms.
> Alarm Level | This indicates the minimum severity level of alarms sent to the remote maintenance center.
> Alarm Suppression | When this is active, no alarms are sent to the remote maintenance center.
> Clear Alarm Notification | When the system reboots, all active alarms are resolved. If the field is Active, an entry indicating that all alarms were cleared is sent to the remote maintenance center
Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.