Search This CD Index Contact Us
Home > Administration > Networking > AMIS Analog Networking > AMIS Analog Networking Administration > System-Parameters Analog-Network Screen
| System-Parameters Analog-Network Screen
> Table: Field Definitions: System-Parameters Analog-Network Screen
> Field | Valid Input | Description
> --- | --- | ---
> CALLBACK NUMBERS | Country: from 0 to 4 digits. Area/Trunk: from 0 to 7 digits. Local Number: from 1 to 15 digits. | Enter the complete telephone number that other systems will use to contact this machine in the `CALLBACK NUMBERS:` fields. The callback number has three parts and must be no more than 15 digits. Under Country, enter the Country Code of the callback number, from 0 to 4 digits. A Country Code of 0 is typically used to indicate that the callback number is a private network number. This field can be left blank. Under Area/Trunk, enter the area code or trunk ID of the callback number, from 0 to 7 digits. Under Local Number, enter the local telephone number of the callback number.
> AMIS Analog Networking Incoming Allowed? | y = yes n = no | Enter y or n in the `AMIS Analog Networking Incoming Allowed?` field to indicate whether incoming AMIS analog calls are accepted by the AUDIX system.
> AMIS Analog Networking Outgoing Allowed? | y = yes n = no | Enter y or n in the `AMIS Analog Networking Outgoing Allowed?` field to indicate whether outgoing AMIS analog calls are allowed on the AUDIX system.
> AMIS Prefix | From 0 to 5 digits | Enter a prefix in the `AMIS Prefix:` field. You might need to specify an AMIS prefix to make AMIS analog addresses unique. If you assign an AMIS prefix, make sure you provide it to users.
> AMIS Protocol—Use 8 Minutes For Incoming Message Length 0? | y = yes n = no | Enter y or n in the `AMIS Protocol—Use 8 Minutes For Incoming Message Length 0?` field. If an incoming message has a length of 0, or an unknown length, it is treated as an 8-minute-long message. If you specify n, messages can be subject to rejection if they are too long.
> AMIS Loopback Test Mailbox Extension | From 0 to 10 digits | If you set up a loopback test mailbox, enter its extension`` in this field. Any message delivered to this special mailbox causes a reply message to be returned to the sending mailbox.
Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.