Search This CD Index Contact Us
Home > Getting Started > Concepts and Features > Platform Descriptions
| Platform Descriptions
This topic provides information about the following components of the platform: Chassis Capacities Processor Voice/fax ports Storage devices Controllers Ports Monitor, keyboard, and mouse Modems Uninterruptible power supply Terminals ### Chassis The platform contains six PCI slots, three of which are used to support up to three analog-line interface cards in a tower configuration. The chassis is equipped with a cooling fan. ### Capacities The INTUITY AUDIX LX system supports call traffic generated by a maximum of 20,000 local and 500,000 remote messaging subscribers. It supports up to 12 analog voice/fax channels and up to 8 networking channels. The system supports 500 hours of storage, as well as up to 1,000 INTUITY Message Manager clients with a maximum of 32 simultaneous sessions. Text-to-speech sessions are limited to four. ### Processor The platform CPU is a 2 GHz Pentium 4 processor and is equipped with 256 MB of RAM. ### Voice/Fax Ports Up to three 4-port analog-line interface cards are supported to provide up to 12 ports of voice and fax. ### Storage Devices The platform is equipped with an IDE hard drive and a CD-RW drive, which is used for software installation and for backups. A portion of the hard disk is reserved for nonspeech data storage, such as data for the LINUX operating system, the INTUITY AUDIX LX system platform executables and data, and the INTUITY AUDIX LX system software executables. This disk area is very important for proper INTUITY system operations and cannot be changed or used for any other purposes. The rest of the hard disk is used for storing messaging components such as voice messages, subscribers' personal greetings, and automated attendant voiced menus. ### Controllers The video controller, LAN controller, and IDE controller reside on the motherboard. ### Ports The platform contains a single parallel port, two serial ports, two USB ports, and one 10/100 Ethernet port. The serial ports can be used for remote diagnostics and serial switch integration, if applicable. The USB ports can be used for an external modem. ### Monitor, Keyboard, and Mouse A monitor, keyboard, and mouse are required for local system operation. A monitor is available for purchase for use with the INTUITY AUDIX LX system. Depending on your location, the keyboard and mouse are provided with the system. Contact your sales representative for more information. ### Modems Access for remote diagnostics is provided through an external modem. A serial modem is provided with the INTUITY AUDIX LX system. A USB modem is also supported and is available for purchase. Contact your sales representative for more information. ### Uninterruptible Power Supply An Uninterruptible Power Supply (UPS) is strongly recommended for use with INTUITY systems. ### Terminals While it is recommended that you use the Web interface to administer the INTUITY AUDIX LX system, you can also administer the system remotely through the use of a modem and one of the following terminals: Avaya 4410 (for PROCOMM PLUS 4410 or Terranova emulation) Avaya 715 Avaya 4425 vt100 (for vt100 or vt131 emulation) Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.