Search This CD Index Contact Us
Home > Getting Started > Installation > Connecting the Analog-line Interface Cards
| Connecting the Analog-line Interface Cards
> This topic provides the basic information you need to connect the analog-line interface cards installed in the INTUITY AUDIX LX system to the switch. The INTUITY AUDIX LX system supports a maximum of three analog-line interface cards. Each card has four RJ-11 jacks on its bracket (see Back View of Platform for reference). Each RJ-11 jack supports one voice channel.
> Damage from electrostatic discharge is possible. See Protecting Against ESD Damage for more information.
To connect the analog-line interface cards to the switch: Plug a phone cable into each RJ-11 jack on the first card. Plug the other end of each phone cable into the switch. Repeat steps 1 and 2 for each installed card. Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.