Search This CD Index Contact Us
Home > Administration > System Administration > Display Voice Equipment Page
| Display Voice Equipment Page
> Table: Field Definitions: Display Voice Equipment page
> Field Name | Description/Procedure
> --- | ---
> `CARD` | Identifies which voice card the channel resides on (0 through 11) and its position on that card (0 through 5). For example, a CD.PT of 1.1 signifies that this is the second voice card, second channel.
> `PORT` | The position of new channel's on the card.
> `CHANNEL` | The channel number. Channels are numbered sequentially beginning with the first voice card (0 through 63).
> `STATE` | The current status of the channel, as follows: In-service (INSERV) - the normal state Facility-out-of-service (FOOS) Manually-out-of-service (MANOOS) Hardware-out-of-service (HWOOS) broken - diagnostics did not pass on the card and it may have to be replaced
> `TIME` | The time and date of the last change in state of the channel.
> `SERVICE` | The associated service name or a DNIS designation indication.
> `PHONE` | The switch extensions that corresponds to the channel.
> `GROUP` | Not applicable.
> `OPTS` | The equipment options (talk or TDM).
> `TYPE` | The type of voice card being used.
Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.