Search This CD Index Contact Us
Home > Maintenance > Alarms > VM (Voice Messaging) Alarms
| VM (Voice Messaging) Alarms
The alarms on this page are generated by the VM application and indicate a problem with the voice messaging system. The VM alarms are organized as follows: VM Alarms (excluding SOFTWARE alarms) VM SOFTWARE Alarms ### VM Alarms (excluding SOFTWARE alarms)
ALARM_ORIG 0 ANNC 4 AUD_BKUP 0 AUDIT 0 AUDIT 1 AUDIT 2 AUDIT 3 AUDIT 100 AUDIT 101 AUDIT 102 AUDIT 103 AUDIT 104 AUDIX_FS 0 AUDIX_FS 1 |  | AUDIX_FS 2 AUDIX_FS 3 AUDIX_FS 4 AUDIX_FS 5 AUDIX_FS 6 AUDIX_FS 7 AUD_RESTOR 0 FAXAP 0 GRAMMAN 001 LANINTF 0 LANINTF 1 LDAPFAIL 0 NAMESTESTR 0 NET_CONN 0 |  | NOCUSTANNC 0 REORGDB 0 REORGDB 1 RPCTEST 001 SERVER 900 SERVER 901 VM_PT 2 VM_PT 3 VM_PT 4 VM_PT 5 VM TRAFIXFAIL 0 VMDIRS 0
### VM SOFTWARE Alarms
SOFTWARE 0 SOFTWARE 1 SOFTWARE 2 SOFTWARE 100 SOFTWARE 101 SOFTWARE 201 SOFTWARE 202 SOFTWARE 203 SOFTWARE 204 SOFTWARE 601 SOFTWARE 6000 SOFTWARE 6001 SOFTWARE 6600 SOFTWARE 6603 SOFTWARE 6604 SOFTWARE 6605 |  | SOFTWARE 6606 SOFTWARE 6607 SOFTWARE 6608 SOFTWARE 6609 SOFTWARE 6610 SOFTWARE 6611 SOFTWARE 6612 SOFTWARE 6613 SOFTWARE 6614 SOFTWARE 6615 SOFTWARE 6616 SOFTWARE 6617 SOFTWARE 6618 SOFTWARE 6619 SOFTWARE 7701 SOFTWARE 7702 |  | SOFTWARE 7703 SOFTWARE 7704 SOFTWARE 7705 SOFTWARE 7706 SOFTWARE 7707 SOFTWARE 7708 SOFTWARE 7709 SOFTWARE 7710 SOFTWARE 7712 SOFTWARE 7713 SOFTWARE 7714 SOFTWARE 7715 SOFTWARE 7716 SOFTWARE 7717 SOFTWARE 7718 SOFTWARE 7719
### VM ALARM_ORIG 0 ##### Description: This alarm indicates a test of Alarm Origination. The remote support center is conducting this test. ##### Repair Procedure: No corrective action is necessary. ### VM ANNC 4 ##### Description: The active announcement set is one of following: Inaccessible Nonexistent Corrupt ##### Repair Procedure: Contact your remote support center. ### VM AUD_BKUP 0 ##### Description: Portions of the INTUITY AUDIX LX system data backup failed.
Note: The system is providing INTUITY AUDIX service, and the current backup is valid. However, future backups may fail.
##### Repair Procedure: Contact your remote support center. ### VM AUDIT 0 ##### Description: The nightly audit failed. ##### Repair Procedure: Contact your remote support center. ### VM AUDIT 1 ##### Description: The delivery data audit failed.
Note: This alarm is probably related to the mailing lists audit.
##### Repair Procedure: Contact your remote support center. ### VM AUDIT 2 ##### Description: The database audit failed. This condition can occur after a move from one switch to another or after a power outage. ##### Repair Procedure: Contact your remote support center. ### VM AUDIT 3 ##### Description: The database audit failed. This condition can occur after a move from one switch to another or after a power outage. ##### Repair Procedure: Contact your remote support center. ### VM AUDIT 100 ##### Description: Portions of the weekly database audit failed. The system is providing INTUITY AUDIX service. This service, however, might be limited or inconsistent. ##### Repair Procedure: Contact your remote support center. ### VM AUDIT 101 ##### Description: The weekly database audit failed. ##### Repair Procedure: Contact your remote support center. ### VM AUDIT 102 ##### Description: Portions of the weekly database audit failed. ##### Repair Procedure: Contact your remote support center. ### VM AUDIT 103 ##### Description: Portions of the weekly database audit failed. ##### Repair Procedure: Contact your remote support center. ### VM AUDIT 104 ##### Description: Portions of the weekly database audit failed. ##### Repair Procedure: Contact your remote support center. ### VM AUDIX_FS 0 ##### Description: The system logs this alarm when the voice storage space used is at 90% capacity or greater. The system automatically resolves this alarm when the space usage drops below 85%.
Note: This condition causes serious subscriber problems.
##### Repair Procedure: Contact your remote support center. ### VM AUDIX_FS 1 ##### Description: The INTUITY AUDIX data space used reached 80% capacity. The system automatically resolves this alarm when the space usage drops below 75%. If the space usage does not decrease, this alarm can escalate to a VM AUDIX_FS 0 alarm. ##### Repair Procedure:
Note: After each step, check for resolved alarms to see if you have freed enough space.
Decrease the maximum number of activity log entries by doing the following: Log in to the INTUITY AUDIX Command Prompt. The system displays the AUDIX Command Prompt after you enter your login. Enter change system-parameters activity-log. Decrease the number in the `Maximum Number of Activity Log Entries` field. Press F3 (Enter) to save the information. Ask subscribers to delete unneeded messages. You might want to do this by using the Broadcast Messages feature. Reduce message retention time by doing the following. Log in to the INTUITY AUDIX Command Prompt. The system displays the AUDIX Command Prompt after you enter your login. Enter change COS cos-number. The cos-number might be any number from 0 through 11. It is strongly recommended that you modify the cos-number that applies to most subscribers. Press F8 (Next Page). Decrease the number in the `Retention Times (days) New, Old,` and`Unopened` fields under `INCOMING MAILBOX.` Decrease the number in the `Retention Times (days) File Cab` and`Delivered/Nondeliverable` fields under ```OUTGOING MAILBOX`. Press F3 (Enter) to save the information. If the alarm is still active,contact your remote support center. ### VM AUDIX_FS 2 ##### Description: The file count reached 80% capacity. This alarm can escalate to VM AUDIX_FS 0. The system automatically resolves this alarm when the file count used goes below 75%. ##### Repair Procedure:
Note: After each step, check for resolved alarms to see if you have freed enough space.
Ask subscribers to delete unneeded messages. You might want to use the Broadcast Message feature. Remove unused local and remote subscribers by doing the following: Log in to the INTUITY AUDIX Command Prompt. The system displays the AUDIX Command Prompt after you enter your login. Enter remove subscriber name. Enter list remote-extension remote machine name. To list the remote machine names, use the list machines command. Look at the `Usage Date` field for each remote subscriber and delete those that are unused by entering remove remote-subscriber remote subscriber extension. Reboot the system to allow the INTUITY AUDIX system to reclaim unused resources. If the alarm is still active,contact your remote support center. ### VM AUDIX_FS 3 ##### Description: An attempt to restart the INTUITY AUDIX application failed because the INTUITY AUDIX database is corrupted. The system is not providing INTUITY AUDIX service. ##### Repair Procedure: Contact your remote support center. ### VM AUDIX_FS 4 ##### Description: The INTUITY AUDIX data files are corrupted. Although the system is providing INTUITY AUDIX service, subscribers might have trouble sending or receiving messages. ##### Repair Procedure: Contact your remote support center. ### VM AUDIX_FS 5 ##### Description: The INTUITY AUDIX data files are corrupted. Although the system is providing INTUITY AUDIX, subscribers may have trouble sending or receiving messages. ##### Repair Procedure: Contact your remote support center. ### VM AUDIX_FS 6 ##### Description: The database might be corrupted. Although the system is providing INTUITY AUDIX service, this condition could lead to severe problems. ##### Repair Procedure: Contact your remote support center. ### VM AUDIX_FS 7 ##### Description: The system is experiencing possible file system corruption. Although the system is providing INTUITY AUDIX service, this condition could lead to severe problems. Nightly and manual backups usually fail while this alarm is active. ##### Repair Procedure: Contact your remote support center. ### VM AUD_RESTOR 0 ##### Description: An INTUITY AUDIX system-data restore failed. The INTUITY AUDIX application will not initialize. ##### Repair Procedure: Contact your remote support center. ### VM FAXAP 0 ##### Description: Queries to the INTUITY FAX Messaging database fail. This alarm indicates a possible database corruption. ##### Repair Procedure: Contact your remote support center. ### VM GRAMMAN 001 ##### Description: INTUITY AUDIX has lost its connection to the dialing server. The lost connection has occurred because the dialing server is down because it was turned off or because of a TCP/IP problem. ##### Repair Procedure: You must wait for the remote support center to fix this problem. The alarm is called in automatically, unless there is another major alarm still active. ### VM LANINTF 0 ##### Description: The system has a resource problem. ##### Repair Procedure: Contact your remote support center. ### VM LANINTF 1 ##### Description: The system has a resource problem. ##### Repair Procedure: Contact your remote support center. ### VM LDAPFAIL 0 ##### Description: An attempt to restart the LDAP Server on the INTUITY AUDIX server failed. ##### Repair Procedure: Contact your remote support center. ### VM NAMESRESTR 0 ##### Description: Recorded subscriber names are not installed on the system. ##### Repair Procedure: To repair this alarm: Stop the messaging software (voice system). Restore the AUDIX names. Start the messaging software (voice system). ### VM NET_CONN 0 ##### Description A digital networking connection failure has occurred. ##### Repair Procedure: To repair the alarm: Verify the system IP address is correct: Start at the Messaging Administration main menu and select TCP/IP Network Configuration. The system displays the Configure Network Addressing page. Verify that the `IP Address` field contains the correct system IP address. If necessary, enter the correct IP address in the `IP Address` field. Delete any unnecessary administered remote machines. For example, delete any unnecessary test machines. See Deleting Remote Machines for more information. If this alarm persists, reboot the system. ### VM NOCUSTANNC 0 ##### Description The system attempted to restore custom announcements; however, no custom announcement set is administered. ##### Repair Procedure: To repair the alarm: Identify an administrative announcement set. Stop the messaging software (voice system). Restore the custom announcement set. Start the messaging software (voice system). ### VM REORGDB 0 ##### Description: The system logs this alarm when AUDIX initialization fails. System initialization is suspended while the database is reorganized. This error can occur in the following circumstances: Power supply is interrupted. AUDIX restarts for a maintenance reason. Someone presses the Reset button. The system automatically resolves this alarm after it reorganizes the database and completes initialization.
Note: Do not press the Reset button. Wait for the system to reorganize the database and initialize.
##### Repair Procedure: Wait for the alarm to automatically clear. Clearance can take up to 2 hours. If the alarm does not clear after this length of time: Contact your remote support center. ### VM REORGDB 1 ##### Description: The system logs this alarm when a database repair fails. This alarm occurs in the following circumstances: Power supply is interrupted. AUDIX restarts for a maintenance reason. Someone presses the reset button. The system automatically resolves this alarm after it reorganizes the database and reinitializes. ##### Repair Procedure: Contact your remote support center to restore the database from a previous backup. ### VM RPCTEST 001 ##### Description: The operating system's RPC processes are not running and cannot be restarted. This results in IMAPI functionality being impaired and INTUITY AUDIX Message Manager and Trusted Server services not being available. Since the system is providing INTUITY AUDIX services, subscribers can use the telephone interface to retrieve messages. ##### Repair Procedure: Contact your remote support center. ### VM SERVER 900 ##### Description: A trusted server exceeded the inactivity timeout period administered on the INTUITY AUDIX System Parameters IMAPI-Options screen. ##### Repair Procedure: Contact your remote support center. ### VM SERVER 901 ##### Description: A trusted server logged an alarm. ##### Repair Procedure: Contact your remote support center. ### VM SOFTWARE 0 ##### Description: An INTUITY AUDIX process failed. ##### Repair Procedure: When this alarm occurs, the INTUITY AUDIX application automatically restarts. This alarm remains active during the restart and is resolved when the INTUITY AUDIX application successfully restarts. If the system does not successfully restart,contact your remote support center. ### VM SOFTWARE 1 ##### Description: An INTUITY AUDIX process failed. ##### Repair Procedure: When this alarm occurs, the INTUITY AUDIX application automatically restarts. This alarm remains active during the restart and is resolved when the INTUITY AUDIX application successfully restarts. If the system does not successfully restart,contact your remote support center. ### VM SOFTWARE 2 ##### Description: An INTUITY AUDIX process failed. ##### Repair Procedure: When this alarm occurs, the INTUITY AUDIX application automatically restarts. This alarm remains active during the restart and is resolved when the INTUITY AUDIX application successfully restarts. If the system does not successfully restart,contact your remote support center. ### VM SOFTWARE 100 ##### Description: An INTUITY AUDIX process failed to restart. ##### Repair Procedure: Contact your remote support center. ### VM SOFTWARE 101 ##### Description: Nonstandard system software is in use. ##### Repair Procedure: Contact your remote support center. ### VM SOFTWARE 201 ##### Description: An INTUITY AUDIX process could not initialize. The system might be providing limited INTUITY AUDIX service. ##### Repair Procedure: When this alarm occurs, the system automatically attempts to restart the failed process. The alarm remains active until the process successfully initializes, and then the alarm is automatically resolved. If this alarm fails to resolve,contact your remote support center. ### VM SOFTWARE 202 ##### Description: An INTUITY AUDIX process could not operate. The system might be providing limited INTUITY AUDIX service. ##### Repair Procedure: When this alarm occurs, the system automatically attempts to restart the failed process. The alarm remains active until the process successfully initializes, and then the alarm is automatically resolved. If this alarm remains active,contact your remote support center. ### VM SOFTWARE 203 ##### Description: An INTUITY AUDIX process failed to initialize. The system might be providing limited INTUITY AUDIX service. ##### Repair Procedure: Contact your remote support center. ### VM SOFTWARE 204 ##### Description: An INTUITY AUDIX process failed during operation. The system might be providing limited INTUITY AUDIX service. ##### Repair Procedure: Contact your remote support center. ### VM SOFTWARE 601 ##### Description: The system detected nonstandard system software in use. ##### Repair Procedure: Contact your remote support center. ### VM SOFTWARE 6000 ##### Description: An INTUITY AUDIX process could not initialize. The system is not providing INTUITY AUDIX service. ##### Repair Procedure: Contact your remote support center. ### VM SOFTWARE 6001 ##### Description: An INTUITY AUDIX process failed to operate. ##### Repair Procedure: Contact your remote support center. ### VM SOFTWARE 6600 ##### Description: The INTUITY AUDIX database automatic rebuild failed. The system is not providing INTUITY AUDIX service. The INTUITY AUDIX application has automatically stopped its own operation and networking and attempted a restart. During this restart, the application operates database file checks and performs a rebuild audit to correct any problems or discrepancies detected. If the rebuild audit is not successful, this system generates this alarm. ##### Repair Procedure: Contact your remote support center. ### VM SOFTWARE 6603 ##### Description: The INTUITY AUDIX application detected file damage during a restart. The system stops the initialization and the software attempts to fix the file problems. The system automatically resolves this alarm after completing the fix and continues initialization. ##### Repair Procedure: Contact your remote support center. ### VM SOFTWARE 6604 ##### Description: The system encountered problems while updating extension length values. Although the system updated the extension length, the INTUITY AUDIX application could not update its internal tables. This alarm can block administrators from adding new subscribers. ##### Repair Procedure: Stop the messaging software (voice system). Start the messaging software (voice system) to synchronize the voice platform and the INTUITY AUDIX application. If the alarm fails to resolve,contact your remote support center. ### VM SOFTWARE 6605 ##### Description: The automated attendant routing table contains inconsistent data. This alarm occurs when a call to an automated attendant cannot be routed as specified. This alarm can occur if the routing tables are not updated after voice mailboxes listed in the table are removed or if file corruption from a system crash occurs. The system automatically resolves this alarm after the table is updated. ##### Repair Procedure: Update the routing tables with correct data. If this alarm persists,contact your remote support center. ### VM SOFTWARE 6606 ##### Description: An automated attendant software failure. When this alarm occurs, the INTUITY AUDIX application can restart or shut down. ##### Repair Procedure: Contact your remote support center. ### VM SOFTWARE 6607 ##### Description: The system has an inconsistent holiday or business schedule name. This alarm occurs when a call to an automated attendant cannot be routed as specified. The system automatically resolves this alarm after a successful restoration of data and voice system restart. ##### Repair Procedure: Restore the system data. ### VM SOFTWARE 6608 ##### Description: The system is experiencing inconsistent automated attendant software operations. ##### Repair Procedure: Contact your remote support center. ### VM SOFTWARE 6609 ##### Description: The system detected inconsistent automated attendant night service data. ##### Repair Procedure: Contact your remote support center. ### VM SOFTWARE 6610 ##### Description: The INTUITY AUDIX application cannot write to the day/night service file. The system is not providing correct night service operation. This alarm might occur with alarm VM SOFTWARE 6609. ##### Repair Procedure: This alarm is automatically resolved when the proper night service state is determined. If this alarm remains active,contact your remote support center. ### VM SOFTWARE 6611 ##### Description: The INTUITY AUDIX application cannot communicate with the voice platform software. The system is providing limited or interrupted INTUITY AUDIX service. ##### Repair Procedure: Contact your remote support center. ### VM SOFTWARE 6612 ##### Description: The INTUITY AUDIX outcalling feature failed. ##### Repair Procedure: Contact your remote support center. ### VM SOFTWARE 6613 ##### Description: An error occurred during system installation, or the system experienced incorrect modifications. System operation might be impaired. ##### Repair Procedure: Contact your remote support center. ### VM SOFTWARE 6614 ##### Description: The system failed to initialize the INTUITY AUDIX application because of insufficient system resources. The system is not providing INTUITY AUDIX service. ##### Repair Procedure: Contact your remote support center. ### VM SOFTWARE 6615 ##### Description: During system initialization, the traffic process is unable to access one of its database files. ##### Repair Procedure: Reboot the system. ### VM SOFTWARE 6616 ##### Description: The AUDIX initialization process detected corrupt traffic data files. The system automatically begins to correct the corruption. ##### Repair Procedure: Contact your remote support center. ### VM SOFTWARE 6617 ##### Description: The INTUITY AUDIX server detects that the LDAP Server is not responding. ##### Repair Procedure: The server attempts to restart the LDAP Server. If the LDAP Server is restarted, the alarm is resolved. If the LDAP Server does not restart, minor alarm VM LDAPFAIL0 are then raised. ### VM SOFTWARE 6618 ##### Description: The system detected a database problem. Stopping and restarting the voice system automatically repairs the database. ##### Repair Procedure: Stop the messaging software (voice system). Start the messaging software (voice system). If the alarm is still active,contact your remote support center. ### VM SOFTWARE 6619 ##### Description: INTUITY AUDIX call processing detected a problem with the LDAP server. ##### Repair Procedure: Reboot the system. ### VM SOFTWARE 7701 ##### Description: The system failed to locate all of the software needed to initialize the INTUITY AUDIX application. The system is not providing INTUITY AUDIX service. This failure can occur after a power hit or when a disk error happens. This alarm is also sent to the remote support center. ##### Repair Procedure: Contact your remote support center. ### VM SOFTWARE 7702 ##### Description: The system found that INTUITY AUDIX database files were missing during AUDIX initialization. The system is not providing INTUITY AUDIX service. This failure can occur after a power hit or when a disk error happens. ##### Repair Procedure: Contact your remote support center. ### VM SOFTWARE 7703 ##### Description: The system experienced an unexpected file check failure after a voice system restart or a reboot. ##### Repair Procedure: Contact your remote support center. ### VM SOFTWARE 7704 ##### Description: The system restarts too often. Because of another alarm, the INTUITY AUDIX application has tried to restart itself twice but has failed. The system is not providing INTUITY AUDIX service. ##### Repair Procedure: Contact your remote support center. ### VM SOFTWARE 7705 ##### Description: The INTUITY AUDIX maintenance software automatically shut down the INTUITY AUDIX application and attempted a restart. This alarm can also indicate that the system attempted too many restarts or that an unexpected error occurred during the shutdown. The system is not providing INTUITY AUDIX service. ##### Repair Procedure: Contact your remote support center. ### VM SOFTWARE 7706 ##### Description: The system rebooted too often. Because of another alarm, INTUITY AUDIX Voice Messaging has tried to restart itself but has failed. The system is not providing INTUITY AUDIX service. ##### Repair Procedure: Contact your remote support center. ### VM SOFTWARE 7707 ##### Description: The INTUITY AUDIX maintenance software automatically shut down the INTUITY AUDIX application and attempted a restart. This alarm can also indicate that the system attempted too many restarts or that an unexpected error occurred during shutdown. The system is not providing INTUITY AUDIX service. ##### Repair Procedure: Contact your remote support center. ### VM SOFTWARE 7708 ##### Description: The system rebooted too many times. Because of another alarm, the INTUITY AUDIX application has tried to restart itself but has failed. The system is not providing INTUITY AUDIX service. ##### Repair Procedure: Contact your remote support center. ### VM SOFTWARE 7709 ##### Description: The INTUITY AUDIX maintenance software automatically shut down the INTUITY AUDIX application and attempted a restart. This alarm can also indicate that the system attempted too many restarts or that an unexpected error occurred during shutdown. The system is not providing INTUITY AUDIX service. ##### Repair Procedure: Contact your remote support center. ### VM SOFTWARE 7710 ##### Description: The maintenance software stopped INTUITY AUDIX operation during a restart. The system is not providing INTUITY AUDIX service. ##### Repair Procedure: Contact your remote support center. ### VM SOFTWARE 7712 ##### Description: The maintenance software has automatically shut down the INTUITY AUDIX application and attempted a restart. The system is not providing INTUITY AUDIX service. ##### Repair Procedure: Contact your remote support center. ### VM SOFTWARE 7713 ##### Description: The system failed to create a new voice file system during INTUITY AUDIX initialization. This problem can occur while an Avaya technician attempts to add additional hours of speech to the system. The system is not providing INTUITY AUDIX service. ##### Repair Procedure: Contact your remote support center. ### VM SOFTWARE 7714 ##### Description: The INTUITY AUDIX outcalling feature failed. The system is providing only limited INTUITY AUDIX service. ##### Repair Procedure: Contact your remote support center. ### VM SOFTWARE 7715 ##### Description: The INTUITY AUDIX trusted server notification feature failed. The system is providing only limited INTUITY AUDIX service. ##### Repair Procedure: Contact your remote support center. ### VM SOFTWARE 7716 ##### Description: The system failed to find the external security password file. Any usage of the old, external security password will fail. If you have one or more external trusted servers, administer a new external security password. ##### Repair Procedure: Do one of the following: If your system does not have one or more external trusted servers,contact your remote support center. If your system has one or more external trusted servers: Log in to the INTUITY AUDIX Command Prompt. The system displays the AUDIX Command Prompt after you enter your login. At the enter command: prompt, enter change imapi-password The system displays the Change IMAPI-Password screen. Complete the `Current Password:` and `New Password:` fields. Press F3 (Enter) to save the change. Enter exit at the `enter command:` prompt. ### VM SOFTWARE 7717 ##### Description: The system failed to find any announcement sets during INTUITY AUDIX initialization. The system is not providing INTUITY AUDIX service. ##### Repair Procedure: Contact your remote support center. ### VM SOFTWARE 7718 ##### Description: During the system initialization, the AUDIX database integrity check failed. The system is not providing service. ##### Repair Procedure: Contact your remote support center. ### VM SOFTWARE 7719 ##### Description: This alarm tells you that the outcalling database is corrupted. ##### Repair Procedure: Contact your remote support center to have them reinitialize the database. Next, have all subscribers re-enter their outcalling database information. ### VM TRAFIXFAIL 0 ##### Description: The automatic file recovery procedure started by VM SOFTWARE 6616 failed. The system will continue to provide service, but traffic collection data is incomplete. ##### Repair Procedure: Contact your remote support center. ### VM VM_PT 2 ##### Description: An INTUITY AUDIX port restart is in progress. ##### Repair Procedure: No corrective action is necessary. ### VM VM_PT 3 ##### Description: An INTUITY AUDIX port process failed too many times. The system set the service status of the affected channel to manually out of service (manoos). ##### Repair Procedure: Contact your remote support center. ### VM VM_PT 4 ##### Description: An attempt to send or receive a fax failed. The system generates this alarm after a number of failures occur. ##### Repair Procedure: The system automatically resolves this alarm if a failure does not reoccur within 5 minutes. If this alarm fails to remains active,contact your remote support center. ### VM VM_PT 5 ##### Description: An attempt to record or print a fax failed. The system generates this alarm after a number of failures occur. This alarm can indicate a problem with the subscribers' fax equipment or INTUITY AUDIX FAX Messaging administration. ##### Repair Procedure: Verify that the subscribers' fax equipment is working properly. Verify that INTUITY FAX Messaging is properly administered. If the alarm fails to resolve,contact your remote support center. ### VM VMDIRS 0 ##### Description: The INTUITY AUDIX application is experiencing problems with a file. Although the system is providing INTUITY AUDIX service, the system response times may be slow and the performance poor. ##### Repair Procedure: Contact your remote support center. Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.