Search This CD Index Contact Us
Home > Administration > Networking > Digital Networking > Digital Networking Administration > Listing Address Ranges for Network Machines
| Listing Address Ranges for Network Machines
The Address Ranges screen displays a numerical list of address ranges that belong to all machines in the network. You can use this screen to determine if you have overlapping address ranges in your network. If you have overlapping address ranges, you need to add a prefix for address ranges on the local or remote Machine Profile screens for any overlapping addresses. To list address ranges: Start at the Messaging Administration main menu and select Messaging. The system then displays the AUDIX Command Prompt after you enter your login. Enter list address-ranges or list address-ranges starting_address at the `enter command:` prompt. The system displays the following message: `Display Only Those Ranges with Maximum Number of Overlaps? n` To display all address ranges for all machines in the network, leave the default at n for no. To display only ranges with the maximum number of overlaps, that is, 16 machines with overlapping address ranges, type y for yes. Press F3 (Enter). The system displays the Address Ranges screen. See the table for Field Definitions: Address Ranges Screen for field descriptions of this display-only screen. Use F7 (NextPage) and F8 (PrevPage) to scroll through the screens, if applicable. Press F1 (Cancel). The cursor returns to the command line, and the system displays the following message: `Command Successfully Completed`. Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.