Search This CD Index Contact Us
Home > Administration > Networking > Digital Networking > Digital Networking Administration > Machine Profile Screen for the Local Machine, Page 2
| Machine Profile Screen for the Local Machine, Page 2
> Table: Field Definitions: Local Machine Profile Screen, Page 2
> Field | Valid Input | Description
> --- | --- | ---
> IP Address | Display-only | The IP address of the local machine.
> Password | From 5 to 10 alphanumeric characters; can include dashes or underscores | Enter the password remote that machines must use to establish networking connections to this local INTUITY system.
> Updates: In? | y = yes n = no | If you enter y, this local INTUITY system accepts updated subscriber database information from any remote machine (the Updates In field must also be set to y on the remote Machine Profile screen setup on the local INTUITY AUDIX system for each remote machine). If you enter n, the local INTUITY AUDIX system does not accept updates from any remote machine, regardless of the entry on the remote Machine Profile screen. Set this field to y only after testing the network end to end during initial administration.
> Updates: Out? | y = yes n = no | If you enter y, updates to subscriber database information for local subscribers are sent to a remote machine (the Updates Out field must also be set to y on the remote Machine Profile screen set up on the local INTUITY system for each remote machine). If you enter n, updates are not sent to any remote machine, regardless of the entry for this field on the remote Machine Profile screen. Set this field to yes only after testing the network end to end during initial administration.
> Allow Automatic Full Updates | y = yes n = no | If you enter y, the local INTUITY system automatically requests full updates from remote systems. If you enter n, the local INTUITY system does not automatically request full updates from remote systems.
Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.