Search This CD Index Contact Us
Home > Administration > ADAP > Installing ADAP
| Installing ADAP
Installation Requirements Recommended Hardware Configurations ADAP Directory Structure ADAP Diskette Contents Installation Procedures Checking config.sys and autoexe.bat Files This topic tells you how to install ADAP software on your PC. This consists of the following three tasks, described in detail later in this topic: Determine that required hardware is in place and configured properly. Understand how the ADAP directories are organized on your PC. Perform the installation. Installation procedures are the same whether you install ADAP for the first time or upgrade from an earlier version of ADAP. ### Installation Requirements Before you install the ADAP software, check that your PC system consists of the following: An IBM-compatible PC with: A minimum of 640 KB of RAM A 3.5" 1.44 MB floppy disk drive One fixed disk (hard drive) with a minimum of 40 MB of storage MS-DOS Note: If you have AUDIX Call Detail Recording (CDR), see the AUDIX Call Detail Recording Package, 585-305-506, for the CDR hardware requirements A PC–compatible, parallel port printer for printing text files. #### Recommended Hardware Configurations Your PC must be connected to the voice mail system through one of the following configurations: Directly, with a Group 311 RS-232 cable connected from your PC to a Group 350 null modem cable, which in turn is connected to: Either Port A on the INTUITY AUDIX system or The local administration terminal (LAT) connector on the back of the AUDIX system An RS-232 cable that cannot not exceed 50 feet Through a switch that uses a Hayes-compatible modem Through a switch that uses Modular Processor Data Module (MPDM) ### ADAP Directory Structure When you install the ADAP software for INTUITY AUDIX, the default directory used by the ADAP setup software is INT_ADAP, unless the ADAPROOT environment variable is set otherwise. After installation is complete, these directories contain the appropriate ADAP software. Since both directories contain programs with the same names, the PATH environment variable indicates which of the two directories is to be used when you execute the ADAP software. You must create the machine directories (<machine1>, <machine2>, etc.) they will contain the data that you retrieve from each voice mail machine using ADAP. If you are working with more than one voice mail machine, you need to create a directory corresponding to each machine. #### ADAP Diskette Contents Each diskette contains a readme file that lists the ADAP files and directories contained on that diskette. To display the contents of the readme file, insert the diskette in drive A and enter type a:readme at the DOS prompt. (If you use a drive other than A, enter it instead.) The ADAP software is contained on the 3-1/2-inch diskettes. ### Installation Procedures Installation procedures are the same whether you are installing ADAP for the first time or upgrading from an earlier version of the ADAP software. To install ADAP, you need to do the following procedures: Install the ADAP software. Verify that the config.sys and autoexec.bat files are set up properly for ADAP. #### Install ADAP Software Complete the following steps to install the ADAP software. Installation automatically builds the required subdirectories if they do not exist already. ADAP software is installed by default to C:\PCIFCE or C:\INT_ADAP. If you want to install to a different subdirectory or drive, insert the following environment variable definition in your autoexec.bat file, and reboot your PC: SET ADAPROOT=<drive>:\<directory> (where <drive> is the drive letter and <directory> is the directory path name) Insert AUDIX Administration and Data Acquisition Software, Disk 1 into your floppy disk drive. At the DOS prompt, enter a: RETURN to change to drive A. (If you use a diskette drive other than drive A, enter that drive letter instead.) Enter setup. You are prompted for your floppy disk drive. Enter your floppy disk drive letter name, or press Enter to default to drive a:. The Setup For AUDIX PC Software menu appears. Press a to select Install ADAP Command Line Software. The Install ADAP Command Line Software screen appears. Press i to select Install. Messages describing installation progress appear. When installation of the disk is finished, if there are more disks to install you are prompted to insert the next disk. Each disk takes about a minute to install. Insert the next disk and press any key to continue. Repeat Step 8 for each diskette requested by the Setup program. When installation is finished, an Installation Complete message appears. Press any key to continue. #### Check config.sys and autoexec.bat Files The installation automatically modifies data in the config.sys and autoexec.bat files. Complete the following steps to ensure that these changes were made: At the DOS prompt, type config.sys to display the contents of the config.sys file. Check for the rs232 device line: device=c:\pcifce\ex_rs232.bin This line identifies the device driver for communicating with the voice mail system. If it is not present, use your text editor to add it to the file. (If you changed the ADAP software subdirectory to a name other than PCIFCE or INT_ADAP, the name you changed it to appears in the file.) Check for the following device line, which tells ADAP how to write things to the screen: device=c:\dos\ansi.sys At the DOS prompt, type autoexec.bat to display the contents of the autoexec.bat file. Check for the line that begins with PATH= and validate the following: c:\pcifce or c:\int_adap If the above entries are not included in your autoexec.bat file, use your text editor to add them to the file. If you made any changes in the previous steps, reboot your system. Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.