Search This CD Index Contact Us
Home > Administration > Networking > Digital Networking > Digital Networking Administration > Machine Profile Screen for the Local Machine, Page 1
| Machine Profile Screen for the Local Machine, Page 1
> Table: Field Definitions: Local Machine Profile Screen, Page 1
> Field | Valid Input | Procedure/Description
> --- | --- | ---
> Machine Name | From 0 to 10 alphanumeric characters; can include dashes or underscores | The name of the local machine. This field cannot contain a period or begin with a digit. The use of the machine name "fax" is reserved and not permitted. Machine names must be unique. Examples: "Chicago", "New York," or "Denver_1." If a machine name includes a space, the name must be enclosed in quotes whenever the name is used in the command line. Example, "New York."
> Machine Type | tcpip | The local machine is always tcpip.
> Location | Display-only | Displays local.
> Voiced Name? | y = yes n = no | This field contains an n until you record a name for the machine. This field automatically changes to y when you record a name for the machine.
> Extension Length | An integer, from 3 through 10 | Enter the length of extensions on the local system. The value you enter must match the extension length in your dial plan.
> Voice ID | Display-only | Displays a system-assigned identifier that you must use to identify the machine if you decide to record machine names.
> Default Community | An integer, from 1 through 15 | If you have administered your system to use community sending restrictions, enter the default community number for your subscriber population.
> Prefix | From 0 to 21 alphanumeric characters | Prefixes can be used on the local machine, but they limit the functionality and are not recommended. For a detailed discussion of the use and implications of prefixes, see Fax Administration.
> Start Ext. | A 3-digit to 10-digit string | Enter the starting extensions for the ranges of telephone numbers used on the local system. (Designate a block of switch extensions that can be used at the local system when you are assigning subscribers.) For example, if your system uses extensions between 2000 and 3000, enter 2000 in the Start Ext. field. Up to 10 different ranges can be specified to pinpoint the exact set of extension blocks that are used by the local system. The length of the start and end extension must agree with the Extension Length field. For a 5-digit extension, the default is from 00000 to 99999.
> End Ext. | A 3-digit to 10-digit string | Enter the ending extensions for the ranges of telephone numbers used on the local system. For example, if your system uses extensions between 2000 and 3000, enter 3000 in the End Ext. field.
> Warnings | Display-only | This field displays a warning when a duplication or overlap of an extension range for another machine is being assigned.
Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.