Search This CD Index Contact Us
Home > Maintenance > Switch Integration Troubleshooting > Example of Additional Tone Page—First Additional Tone
| Example of Additional Tone Page—First Add Tone
> ##### Table: First Additional Tone Page— Field Descriptions
> Field | Description | Values
> `Frequency 1 and 2` | This field refers to the set of frequencies that are used within each tone. | If a dial tone is 440 Hz + 480 Hz, you need to enter 440 under Frequency 1 and 480 under Frequency 2.
> On Time | Specifies the duration of the On cycles in milliseconds. |
> Off Time | Specifies the duration of the Off cycles in milliseconds. |
> Repetition Count | These fields display the results of analysis of the number of occurrences of the on time/off time cycles. | integer
> `Report as:` | This field is displayed on the additional tones page only. This field takes the value of the Basic Tone type of either Dial, Busy, Ring, or Reorder Tone, and reports the value to the system. If the additional tone is not used, this field takes the value of "unused." | Busy Dial Ringback Reorder Unused
Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.