Search This CD Index Contact Us
Home > Administration > Reports > Network Load Hourly Traffic Screen, Page 2
| Network Load Hourly Traffic Screen, Page 2
> Table: Field Definitions: Network Load Hourly Screen, Page 2
> Field Name | Description/Procedure
> --- | ---
> Date: | The starting date for which traffic data was collected for the report. It is the date you entered on the command line or the current date if you did not specify a date. If you enter a date previous to the current date, each day's record is presented as an additional page (screen). Press F7 (NextPage) and F8 (PrevPage) to scroll through each daily report record.
> Hour: | The starting hour for which traffic data was collected for the report. It is the hour you entered on the command line or the current hour if you did not specify an hour.
> Ending Time: | The time at which data collecting ended.
> NETWORK CHANNEL
> Number: | This maximum available nodes for an INTUITY AUDIX LX.
> Type: | The administered networking channels. If the network channel type is administered during the record collection period, the new channel type is shown.
> USAGE (SECONDS)
> Incoming Outgoing Total | The number of seconds that each network channel was active with incoming and outgoing calls during the recording period. The total seconds of activity are also provided.
> PEG COUNT (NUMBER OF CALLS)
> Incoming Outgoing Total | The number of incoming and outgoing calls on each network channel during the recording period. The total number of calls is also provided.
Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.