Search This CD Index Contact Us
Home > Getting Started > Installation > Installation Prerequisites
| Installation Prerequisites
> INTUITY AUDIX LX Release 2.0 supports the S3210R server. This server replaces the S3210 server for RoHS compliance reasons. The S3210R chassis is designed to be installed in a rack-mount configuration, or in a stackable desktop configuration. This topic covers the following items: Intended audience Safety and security alert labels General precautions FCC statement DOC interference information Site preparation Environmental considerations Installation area considerations Customer-provided cabinet requirements Weight and space considerations Power requirements Grounding requirements Shipment Contents Saving Packing Materials # Intended audience This book is intended primarily for the on-site technical personnel who are responsible for installing the system and performing initial administration and acceptance testing. However, the General Precautions are intended for both installers and system administrators. # Safety and security alert labels This book uses the following symbols to call your attention to potential problems that could cause personal injury, damage to equipment, loss of data, service interruptions or breaches of toll fraud security. CAUTION: indicates the presence of a hazard that if not avoided can or will cause minor personal injury or property damage, including loss of data. WARNING: indicates the presence of a hazard that if not avoided can cause death or severe peronal injury. DANGER: indicates the presence of a hazard that if not avoided will cause death or severe personal injury. # General Precautions
> NOTE: The following applies for system installations in Sweden, Finland and Norway only. The system relies on a ground connection through the main plug with an earth contact. Because of unreliable earthing concerns in Sweden, Finland and Norway, the system must be installed by Service Personnel in a restricted access location. A restricted access location is defined as access that can be gained by only Service Personnel or Customers who have been instructed about the reasons for the restricted access and any safety precautions that must be taken. In these cases, access to the system is gained by the use of a tool (such as a lock and key) or other means of security.
> Lithium battery(ies) included with this system. Do not puncture, mutilate, or dispose of battery(ies) in fire. Danger of explosion if battery is incorrectly replaced. Replace only with the same or equivalent type recommended by manufacturer. Dispose of used batteries in accordance with the manufacturer's instructions and your local regulations.
> ATTENTION: Il y a danger d’explosion s’il y a remplacement incorrect de la batterie. Remplacer uniquement avec une batterie du même type ou d’un type équivalent recommandé par le constructeur. Mettre au rebut les batteries usagées conformément aux instructions du fabricant. # FCC statement This equipment has been tested and found to comply with the limits for a Class A digital device, pursuant to Part 15 of the FCC rules. These limits are designed to provide a reasonable protection against harmful interference when th e equipment is operated in a commercial environment. This equipment generates, uses and can radiate radio-frequency energy and, if not installed and used in accordance with the instruction manual, may cause harmful interference to radio communications. Operation of this equipment in a residential area is likely to cause harmful interference in which case the user will be required to correct the interference at his/her own expense. # DOC interference information This digital apparatus does not exceed the Class A limits for radio noise emissions set out in the radio interference regulations of the Canadian Department of Communications. Le présent appareil nomérique n’émet pas de bruits radioélectriques dépassant les limites applicables aux appareils numériques de la Class A préscrites dans le reglement sur le brouillage radioélectrique édicté par le ministère des Communications du Canada. # Site preparation This section describes physical requirements for the installation site, which include: Environmental considerations Installation area considerations Customer-provided cabinet requirements Weight and space considerations Power requirements Grounding requirements ## Environmental considerations Place the system in an area where the environmental conditions shown in the following table are maintained.
> Operating State | Temperature | Humidity (noncondensing)
> Operating | +10 to +35ºC (+50 to +95ºF) | 20 to 80%, relative humidity
> Non-operating (in storage or being shipped) | -20 to +50ºC (-4 to+122ºF) | 20 to 90%, relative humidity
> ## Installation area considerations
> Observe the following when determining where to place the system: Use only the power cord assembly provided to connect the system to an AC outlet. Install the system within 6 feet (2m) of a grounded AC outlet. Do not use extension cords with the system. Ensure that the AC outlet to be used to power the system (via the power cord) is a grounded outlet. If you are unsure of the ground integrity of the outlet, have a trained and certified electrician check the outlet. Consider the server connection to a branch circuit with regard to overload or overcurrent protection. Verify the system ratings to ensure that, together with other equipment connected to the same branch circuit, an overcurrent or overload condition does not exist. Maintain an air-distribution system that provides adequately cooled, filtered and humidity-controlled air. Do not install the system such that the ventilation or fan openings will be blocked.
> NOTE: The following applies for system installations in Sweden, Finland, and Norway only. The system relies on a ground connection through the main plug with an earth contact. Because of unreliable earthing concerns in Sweden, Finland and Norway, the system must be installed by Service Personnel in a restricted access location. A restricted access location is defined as access that can be gained by only Service Personnel or Customers who have been instructed about the reasons for the restricted access and any safety precautions that must be taken. In these cases, access to the system is gained by the use of a tool (such as a lock and key) or other means of security.
> ## Customer-provided cabinet requirements If you are installing an S3210R in a rack-mounted configuration, the customer-provided cabinet must meet the following requirements: The cabinet must contain a 4-post rack to support the server’s weight. The cabinet must be secured to the floor before attempting to mount any units. The cabinet must accommodate the sliding rails and extender brackets provided with each server. These sliding Rails and extender brackets are designed for mounting in cabinets 22.5 to 32 inches in depth. The cabinet height must accommodate the number of units to be mounted. See Weight and space considerations for server dimensions. ## Weight and space considerations The following table lists the approximate weight, size, and depth of the S3210R system.
> Table: System Weight and Space Considerations
> Weight | Height | Width | Depth
> --- | --- | --- | ---
> 41.5 lb (18.3 kg) | 7 in. (17 cm) | 17 in. (43.3 cm) | 20.5 in. (52 cm)
> Add 3 inches (7.6 cm) to accommodate a rear chassis cable support bracket. If required, add 4 inches (10.2 cm) to accommodate 356B adapter and mounting clip.
> The following table lists the approximate weight, size, height, and depth for the monitor, and keyboard.
> Table: Peripheral Weight and Space Considerations
> Peripheral | Weight | Height | Width | Depth
> --- | --- | --- | --- | ---
> Monitor | 7.1 lb (3.2 kg) | 14 in. (35 cm) | 13.5 in. (34 cm) | 6 in. (15 cm)
> Keyboard | 5 lb (2.3 kg) | 2.5 in. (6.4 cm) | 19 in. (48 cm) | 8 in. (20.5 cm)
> A monitor is not necessarily ordered and shipped for each system. The weight and space considerations listed are for those shipments that include a 15-inch monitor.
> ## Power Requirements for the S3210 Platform of INTUITY AUDIX LX The following table lists the power requirements for the system.
> Attribute | Requirement
> --- | ---
> Volts AC (VAC) | 90–240 (auto-sensing)
> Hertz (Hz) | 47-63 (+/- 3 Hz)
> Phase | Single
> Amps (115V/230V) | 6/3
> Heat Dissipation | 1123 BTU
> In addition to the above power requirements, you must also: Locate each unit within 6 feet (2 meters) of its power receptacle. Keep the communication cables separate from the power cables. Install communication and power cables in accordance with National Electrical Codes (NEC).
> Use only shielded cables and equipment in conjunction with the system to maintain safe levels of electromagnetic compatibility.
> - ## Grounding requirements An S3210R server relies on the ground connection through the main socket-outlet for continued safe operation. Ensure that the AC outlet to be used to power the system (via the UPS or power cord for separate components) is a grounded outlet. If you are unsure of the ground integrity of the outlet, have a trained and certified electrician check the outlet. In addition, observe the following grounding requirements when determining where to place the server: Use only the power cord provided with each unit to connect it to the universal power supply (UPS) or to an AC outlet. Install the server within 6 feet (2 m) of a grounded AC outlet. Do not use extension cords with the system. Use only shielded cables and equipment in conjunction with the system to maintain safe levels of electromagnetic compatibility. WARNING: The servers must be connected to an earthed mains socket-outlet. Failure to do so will result in allowing a hazard to be present that could cause severe personal injury or death. CAUTION: System grounding must comply with the general rules for grounding provided in article 250 of the National Electrical Code (NEC), National Fire Protection Agency (NFPA), or the applicable electrical code in the country of installation. ## Shipment Contents The customer should have received boxes containing the computer, keyboard, and monitor (if ordered). Be sure that you have the following items packed in the box or boxes: The system chassis. Turn out the stablizing feet on the bottom of the computer case. One 6-foot to 8-foot (2-meter to 3-meter) power cord (depending on country in which you are doing the installation) One keyboard with on-board mouse and split connector cord One 4-pin RJ11 cable for each voice port purchased One LAN cable One monitor and power cord, if ordered One Maintenance Modem, and required cables ## Saving Packing Materials Save the shipping carton and all packing materials to use in case you have to return the system to the manufacturer. If you ordered multiple systems, saving one carton and one set of packing materials should be sufficient. Packing materials include: Antistatic bags Cardboard and foam inlays
>   Note: The packing materials also may include a plastic bag designed to protect the system from moisture during shipment. Discard this bag. It is not reusable.
Also save the shipping cartons for the keyboard and monitor. Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.