Search This CD Index Contact Us
Home > Administration > Networking > AMIS Analog Networking > AMIS Analog Networking Administration > Administering the Local Machine
| Administering the Local Machine
> This topic provides information on administering the local INTUITY machine for AMIS. Do not start the AMIS network administration until the local Avaya INTUITY voice messaging system is operating.
> Security Risk! To minimize unauthorized long distance calls, restrict the AMIS Analog Networking and Message Delivery features to send messages only to telephone numbers located in specific calling areas or to specific destinations needed to conduct business. Additionally, use the Message Sending Restrictions feature to administer which subscribers can send AMIS analog networking and message delivery messages and to which locations they can send messages.
## To verify that the local machine is administered correctly for AMIS: Log in to the INTUITY AUDIX Command Prompt. The system displays the AUDIX Command Prompt after you enter your login. Enter change machine at the `enter command:` prompt. The system displays the Local Machine Profile screen. Check the following fields on the screen: `Prefix`: This field is not typically used for the local machine. `Extension Ranges`: These extension ranges must not overlap with planned AMIS/message delivery addresses. Press F1 (Cancel). Continue with Administering a Loopback Test Mailbox (Optional) if you want to administer a loopback test mailbox. If you do not want to administer a loopback test mailbox, continue with Administering Message Delivery Parameters. Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.