Search This CD Index Contact Us
Home > Maintenance > Voice Equipment Diagnostics > Testing a Voice Port
| Testing a Voice Port
> To test a voice port without removing the analog-line interface card from service: Start at the Messaging Administration main menu and select:
>      Voice Port Loop Around
The system displays the Voice Port Loop Around Test page. Complete the fields on the page. For more information, click the field names or Help on the web-based administration page. Click Test. The system completes the diagnostics and displays the Voice Port Loop Around Test Results page. The results page indicates whether each test passed or failed. The result of "not tested" appears next to any test you did not select under Test Type on the Voice Port Loop Around Test page. Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.