Search This CD Index Contact Us
Home > Administration > Networking > AMIS Analog Networking > AMIS Analog Networking Administration > Administering Outcalling Periods
| Administering Outcalling Periods
The AMIS Analog Networking and Message Delivery features use the outcalling ports to deliver messages. To administer outcalling periods: Log in to the INTUITY AUDIX Command Prompt. The system displays the AUDIX Command Prompt after you enter your login. At the `enter command:` prompt, enter change system-parameters outcalling. The system displays the System-Parameters Outcalling screen. Enter y or n in the `Outcalling Active?` field. Enter a start time in the `Start Time` field. Enter an end time in the `End Time` field. Enter the maximum number of ports in the `Maximum Simultaneous Ports` field. Enter the number of minutes, from 0 to 60, that must elapse after a message is delivered before the first outcall occurs in the Initial Delay field. You can use this field to avoid immediately attempting to call users who just received call-answer messages because they were busy or did not answer their phones. Enter a maximum number of digits that can be specified for outcalling in the Maximum Number Digits field. Press F3 (Enter). Continue with Adjusting the System Limits. Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.