Search This CD Index Contact Us
Home > Getting Started > Installation > Activating Alarm Origination
| Activating Alarm Origination
> Note: Complete this step if your location is outside of the United States. Installations inside the United States are set up automatically for alarm origination by the Remote Service Center.
> Do not activate alarm origination for MERLIN LEGEND integrations unless the customer has purchased the optional alarm origination feature.
> Activating alarm origination causes a remote location, such as the remote service center, to receive notification of alarms that occur on the INTUITY AUDIX LX system. Notification can only occur if the Maintenance Modem has been installed. See Connecting the Modem or Activating the Modem for more information. To administer the Alarm Management page: Clear all alarms. Check the CD drive for a CD-RW (at least 4x speed). If the drive does not contain a CD-RW for the nightly backup, insert a labeled CD-RW into the drive.
> Do not activate Alarm Origination unless the CD drive contains a back-up CD-RW.
> 4. Go to the Administration main menu and select Alarm Configuration. The system displays the Configure Alarms page. Type the product ID number in the `Product ID` field.
>    The product ID is always a 9-digit number beginning with the number 2. Do not continue without the correct product ID number.
Select the type of alarm from the `Alarm Origination` drop-down list. Verify that the entry in the `Alarm Suppression` field is `inactive`. If it is not, select `inactive` from the drop-down list. Make other selections as needed. Click the field names or the Help button to see complete field descriptions. Click Save. The system displays an information screen and the following message: `The alarm form has been updated.` Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.