Search This CD Index Contact Us
Home > Maintenance > TCP/IP Diagnostics > Viewing LAN Packet Statistics > View Packet Statistics - TCP/IP Diagnostics Page (Interfaces Statistics Option)
| View Packet Statistics - TCP/IP Diagnostics Page (Interfaces Statistics Option)
> Table: Interface Statistics
> Column | Description
> --- | ---
> Iface | The name of the interface.
> MTU | The maximum transfer unit of the interface.
> MET | The routing metric of the interface.
> RX-OK | The total number of received packets.
> RX-ERR | The number of bad packets received.
> RX-DRP | The number of dropped packets (no space in Linux buffers).
> RX-OVR | The number of received fifo overruns.
> TX-OK | The total number of transmitted packets.
> TX-ERR | The number packet transmit problems.
> TX-DRP | The number of dropped packets (no space in Linux buffers).
> TX-OVR | The number of transmitter FIFO overruns.
> Flg | The flags for an interface: A: Receive all multicast packets B: Broadcast address is valid D: Debugging is on L: Loopback interface M: Receive all packets N: Avoid use of trailers O: No address resolution protocol P: Interface is point-to-point link R: Resources are allocated U: Interface is up
Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.