Search This CD Index Contact Us
Home > Administration > Basic Messaging Administration > System-Parameters Features Screen, Page 2
| System-Parameters Features Screen, Page 2
Table: Field Definitions: System-Parameters Features Screen, Page 2
Field Name | Valid Input | Description/Procedure
MISCELLANEOUS PARAMETERS
Broadcast Mailbox Extension: | Default: blank | The extension number of the system broadcast mailbox. To create a broadcast mailbox, see Setting Up a Broadcast Mailbox.
System Prime Time, Start: End: | 24-hour clock time in the format hh:mm Defaults: Start = 8:00 End = 17:00 | The starting time for the prime-time interval for traffic collection and multiple personal greetings. (This is normally the time your company opens for business.) The ending time for the prime-time interval for traffic collection and multiple personal greetings. (This is normally the time your company closes.)
Increment (l/s), Rewind: Advance: | Default: s = short l = long | s sets the rewind and advance amounts to 4 seconds; l sets the amounts to 10 seconds. Used when a subscriber wants to: Repeat the previous few seconds of the message (press 5) Advance the message (press 6)
FEATURE ACTIVATION
Traffic Collection? | y = yes n = no (Default:y) | Enables or disables the collection of traffic data.
Name Record by Subscriber? | y = yes n = no (Default: y) | Allows or disallows subscribers to from recording their own names.
Multiple Personal Greetings? | y = yes n = no (Default: y) | Enables or disables the multiple personal greetings feature. The multiple personal greetings feature is applied to the entire system.
End of Message Warning? | y = yes n = no (Default: y) | Enables or disables the end of message warning feature.
Warning Time (seconds): | Default: 15 0 = no warning | The number of seconds before the end of the allotted message recording time, when the end of message warning prompt plays.
Priority on Call Answer? | y = yes n = no (Default: y) | Allows or disallows callers to designate a call answer message priority. Callers can designate the message as private, regardless of this setting.
Call Answer Disable? | y = yes n = no (Default: n) | Allows or prevents subscribers to disable call answer. If activated, callers hear the subscriber's greeting but cannot leave a message. Subscribers are addressed to record appropriate instructions in their personal greetings so that callers can understand the options.
Address Before Record? | y = yes n = no (Default: n) | Enables or disables the system to prompt subscribers to address a message before recording. Subscribers who ignore the prompt can still edit the address list after they create the message.
MULTIMEDIA PARAMETERS
Text to Speech Conversion: | Up to 24 alphanumeric characters | Determines which portions of an email message or Message Manager text message the system converts to speech. Subscribers hear a voiced rendition of the selected portion when they access their AUDIX mailboxes. See Setting Text-to-Speech Parameters for more information. headers and body converts the headers and the entire message text.
Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.