Search This CD Index Contact Us
Home > Maintenance > Switch Integration Troubleshooting > Example of a Tones Administration Page—Dial Tone
| Example of a Tones Administration Page—Dial Tone
> Table: OPCODE Commands
> Command | Description
> --- | ---
> OFFHK CH_No. | Seizes the specified line.
> ONHK CH_No. | Emulates an on-hook condition on the specified line (Idle).
> DIAL CH_No. digit_string | Dials out DTMF digits through the specified line.
> FLASH CH_No. duration | Performs hook flash on the channel for the specified number of msec.
> LEARN and Channel number | Captures the PCM data of the voice and performs an analysis of the tone and displays the result.
> WAIT CH_No. duration | Introduces a number of seconds of delay in execution of the next command. This command can be introduced anywhere in the command sequence.
Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.