Search This CD Index Contact Us
Home > Administration > Networking > Digital Networking > Digital Networking Administration > Testing the Digital Networking and TCP/IP Connection > Transmitting Test Packets
| Transmitting Test Packets
> To transmit test packets: Go to the Messaging Administration main menu and select Ping Another Server. The system displays the Send and Receive Test Packets To & From page. Type the internet protocol (IP) address of the system for which you want to run the test in the `IP Address:` field. Click Ping Test to run the test. When the test is finished, the system displays theTest Packets Results page—Internal Test page.
> Note: This page is an example only. The test results displayed for your system will not match those shown here. Examine the test results that are displayed around the midpoint of the window.
Evaluate the results and proceed as follows: If the results show 0% packet loss, continue with Verifying the IP Address for Remote Machines. If the results show 100% packet loss, continue with Correcting Diagnostic Failures for the Avaya INTUITY System. Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.