Search This CD Index Contact Us
Home > Administration > Reports > Network Load Daily Traffic Screen, Page 2
| Network Load Daily Traffic Screen, Page 2
> Table: Field Definitions: Network Load Daily Traffic Screen, Page 2
> Field Name | Description/Procedure
> --- | ---
> NETWORK CHANNEL
> Number | The maximum available nodes for an INTUITY AUDIX LX system.
> Type: | The administered networking channels. If the network channel type is administered during the record collection period, the new channel type is shown.
> USAGE (SECONDS)
> Incoming Outgoing Total | The number of seconds that each network channel was active with incoming and outgoing calls during the recording period. The total seconds of activity are also provided.
> PEG COUNT (NUMBER OF CALLS)
> Incoming Outgoing Total | The number of incoming and outgoing calls on each network channel during the recording period. The total number of calls is also provided.
Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.