Search This CD Index Contact Us
Home > Administration > Networking > Digital Networking > Digital Networking Administration > Machine Profile Screen for a Remote Machine, Page 2
| Machine Profile Screen for a Remote Machine, Page 2
> Table: Field Definitions; Remote Machine Profile Screen, Page 2
> Field | Valid Input | Description
> --- | --- | ---
> IP Address | Four decimal numbers written in dotted format: each number needs to be in the range 0 to 255. For example, 135.9.52.45. | The IP address that is used when AUDIX connects to the remote machine to establish a call for digital networking.
> Password | From 5 to 10 alphanumeric characters; can include dashes or underscores | The password sent to the remote machine when establishing a connection.
> Updates: In? | y= yes n = no | Enter y if the local system accepts updated database information from the remote system (the Updates In field must also be set to y on the local Machine Profile screen). Set to y only after testing the network end to end during initial administration.
> Updates: Out? | y= yes n = no | Enter y if the local system sends updated database information to the remote system (the Updates Out field must also be set to y on the local Machine Profile screen). Set to y only after testing the network end to end during initial administration.
> Send to Non- Administered Recipients? | y= yes n = no | Enter y if the system attempts to deliver messages to nonadministered remote recipients. Enter n if messages cannot be sent to nonadministered recipients.
Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.