Search This CD Index Contact Us
Home > Administration > Networking > AMIS Analog Networking > AMIS Analog Networking Administration > Administering Retransmission Intervals
| Administering Retransmission Intervals
To administer the intervals at which the local system makes delivery attempts: Log in to the INTUITY AUDIX Command Prompt. The system displays the AUDIX Command Prompt after you enter your login. At the `enter command:` prompt, enter change system-parameters features. The system displays the System-Parameters Features screen. Press F7 (Next Page) twice to display page 3. Move the cursor to the `RESCHEDULING INCREMENTS FOR UNSUCCESSFUL MESSAGE DELIVERY` field. Enter a number for the amount of time the local system waits before attempting to retransmit messages, in the `Incr 1:` through `Incr 10:` fields. Press F3 (Enter). Continue with Activating the AMIS Feature Parameter Changes. Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.