Search This CD Index Contact Us
Home > Administration > Networking > Digital Networking > Digital Networking Administration > Adding a Remote Digital Networking Machine
| Adding a Remote Digital Networking Machine
> You can add remote machines during initial system administration or at any time, as your network grows. This topic provides instructions for adding remote machine information on the local machine.
> Note: The INTUITY AUDIX LX system accepts only one local machine. Do not attempt to add a second local machine. Use the instructions in this section only to add remote machines.
To add a remote machine to the local system: Start at the Messaging Administration main menu and select Messaging. The system then displays the AUDIX Command Prompt screen after you enter your login. Enter add machine at the `enter command:` prompt. The system displays the Remote Machine Profile screen, page 1. Complete the fields in this window by using the information provided in the table for Field Definitions: Remote Machine Profile screen, page 1. Press F7 (NextPage). The system displays Remote Machine Profile screen, Page 2. Complete the fields in this window using the information provided in the table for Field Definitions: Remote Machine Profile screen, page 2. Press F3 (Enter) to save the information. The cursor returns to the command line, and the system displays the following message: `Command Successfully Completed`. Press F6 (Cancel) to return to the command line. Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.