Search This CD Index Contact Us
Home > Maintenance > Analog Networking Diagnostics
| Analog Networking Diagnostics
> 1. This topic provides information on performing an AMIS analog networking trace and viewing the networking trace log. To perform an AMIS analog networking trace: Start at the Messaging Administration main menu and select under Messaging Administration:
>        Messaging
Enter your login. The system then displays the AUDIX Command Prompt screen. Enter trace. The system displays the AMIS Trace Activation screen. In the `AMIS-TRACE Activated?` field, enter y. In the `Trace Level:` field, enter one of the following choices: full to trace errors, protocol, and touchtone information normal to trace errors and protocol error to trace errors Press F3 (Enter). Enter another administrative command at the `enter command:` prompt. To view the AMIS analog networking trace log: Start at the AUDIX Command Prompt screen and: Enter display amis-trace The system displays the AMIS Trace Log Display Selection screen. In the `Start Date:` field, enter the date for which you want to view the log. In the `Time:` field, enter the time for which you want to view the log. In the `Search String:` field, enter any words for which you would like to search. Press F3 (Enter). The system displays the AMIS Trace Log screen. Enter another administrative command at the `enter command:` prompt, if desired. Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.