Search This CD Index Contact Us
Home > Maintenance > Getting Inside the Platform > Replacing the PC Cover
| Replacing the PC Cover
Complete the following procedure to replace the PC cover. To replace the PC cover: Carefully set the PC upright if it is not already. Place the side cover on the chassis, aligning the cover with the guides, and then slide the cover into place. When the cover is properly seated, the handle lies flat. Replace the retaining screw that secures the side cover. Set the top cover on the top of the chassis, align the cover with the guides, insert the cover lock through the slot in the top cover, and then slide the top cover into place. Replace the thumb retaining screw at the back of the front cover. Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.