Search This CD Index Contact Us
Home > Administration > Networking > TCP/IP > Administering TCP/IP LAN Connectivity > Attaching the LAN Cable
| Attaching the LAN Cable
> 1. To attach the LAN cable: Shut down the system.
>    Note: The LAN cable used must be a CAT5 cable.
Attach the LAN cable to the LAN connector on the Avaya INTUITY system. Reboot the system. Continue with Testing the TCP/IP Connection or, if you are done, click Return to Main. Top of page

| Search This CD Index Contact Us
| © 2002-2007 Avaya Inc. All rights reserved.